Instalación
Tipos de recursos
Installing/Configuring
PHP Manual

## Configuración en tiempo de ejecución

El comportamiento de estas funciones está afectado por los valores definidos en php.ini.

Exif supports automatically conversion for Unicode and JIS character encodings of user comments when module mbstring is available. This is done by first decoding the comment using the specified characterset. The result is then encoded with another characterset which should match your HTTP output.

Exif configuration options
Name | Default | Changeable | Changelog
--- | --- | --- | ---
exif.encode_unicode | "ISO-8859-15" | PHP_INI_ALL | Available since PHP 4.3.0.
exif.decode_unicode_motorola | "UCS-2BE" | PHP_INI_ALL | Available since PHP 4.3.0.
exif.decode_unicode_intel | "UCS-2LE" | PHP_INI_ALL | Available since PHP 4.3.0.
exif.encode_jis | "" | PHP_INI_ALL | Available since PHP 4.3.0.
exif.decode_jis_motorola | "JIS" | PHP_INI_ALL | Available since PHP 4.3.0.
exif.decode_jis_intel | "JIS" | PHP_INI_ALL | Available since PHP 4.3.0.

For further details and definitions of the PHP_INI_* modes, see the En dónde puede definirse un valor de configuración.

A continuación se presenta una corta explicación de las directivas de configuración.

`exif.encode_unicode` string

  exif.encode_unicode defines the characterset UNICODE user comments are handled. This defaults to ISO-8859-15 which should work for most non Asian countries. The setting can be empty or must be an encoding supported by mbstring. If it is empty the current internal encoding of mbstring is used.

`exif.decode_unicode_motorola` string

  exif.decode_unicode_motorola defines the image internal characterset for Unicode encoded user comments if image is in motorola byte order (big-endian). This setting cannot be empty but you can specify a list of encodings supported by mbstring. The default is UCS-2BE.

`exif.decode_unicode_intel` string

  exif.decode_unicode_intel defines the image internal characterset for Unicode encoded user comments if image is in intel byte order (little-endian). This setting cannot be empty but you can specify a list of encodings supported by mbstring. The default is UCS-2LE.

`exif.encode_jis` string

  exif.encode_jis defines the characterset JIS user comments are handled. This defaults to an empty value which forces the functions to use the current internal encoding of mbstring.

`exif.decode_jis_motorola` string

  exif.decode_jis_motorola defines the image internal characterset for JIS encoded user comments if image is in motorola byte order (big-endian). This setting cannot be empty but you can specify a list of encodings supported by mbstring. The default is JIS.

`exif.decode_jis_intel` string

  exif.decode_jis_intel defines the image internal characterset for JIS encoded user comments if image is in intel byte order (little-endian). This setting cannot be empty but you can specify a list of encodings supported by mbstring. The default is JIS.

Instalación
Tipos de recursos
Installing/Configuring
PHP Manual