printer_draw_bmp
printer_draw_elipse
Printer Functions
PHP Manual

# printer_draw_chord

(PECL printer CVS)

printer_draw_chord — Draw a chord

### Descripción

void printer_draw_chord ( resource `$printer_handle` , int `$rec_x` , int `$rec_y` , int `$rec_x1` , int `$rec_y1` , int `$rad_x` , int `$rad_y` , int `$rad_x1` , int `$rad_y1` )

The function simply draws an chord.

### Lista de parámetros

`printer_handle`

  `printer_handle` must be a valid printer handle.

`rec_x`

  `rec_x` is the upper left x coordinate of the bounding rectangle.

`rec_y`

  `rec_y` is the upper left y coordinate of the bounding rectangle.

`rec_x1`

  `rec_x1` is the lower right x coordinate of the bounding rectangle.

`rec_y1`

  `rec_y1` is the lower right y coordinate of the bounding rectangle.

`rad_x`

  `rad_x` is x coordinate of the radial defining the beginning of the chord.

`rad_y`

  `rad_y` is y coordinate of the radial defining the beginning of the chord.

`rad_x1`

  `rad_x1` is x coordinate of the radial defining the end of the chord.

`rad_y1`

  `rad_y1` is y coordinate of the radial defining the end of the chord.

### Valores retornados

No value is returned.

### Ejemplos

Example #1 printer_draw_chord() example

`<?php
$handle = printer_open();
printer_start_doc($handle, "My Document");
printer_start_page($handle);
$pen = printer_create_pen(PRINTER_PEN_SOLID, 2, "000000");
printer_select_pen($handle, $pen);
$brush = printer_create_brush(PRINTER_BRUSH_SOLID, "2222FF");
printer_select_brush($handle, $brush);
printer_draw_chord($handle, 1, 1, 500, 500, 1, 1, 500, 1);
printer_delete_brush($brush);
printer_delete_pen($pen);
printer_end_page($handle);
printer_end_doc($handle);
printer_close($handle);
?>`

printer_draw_bmp
printer_draw_elipse
Printer Functions
PHP Manual